Lock System Comparison
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	Pulse / Pulse Next
2 users
	Pulse / Pulse Next
10 users
	Pulse PRO
	DigiTech
	MiniTech
	TechMaster

	Power Supply
	9V Battery
Large Battery Box
12V power supply
	9V Battery
Large Battery Box
12V power supply
	9V Battery
Large Battery Box
12V power supply
	9V Battery
Large Battery Box
12V power supply
	9V Battery
Large Battery Box
12V power supply
	9V Battery
Large Battery Box
12V power supply

	Users
	· 1 Manager
· 1 User
	· 1 Manager
· 8 Users
	· Up to 2 Masters
· Up to 2 Managers
· Up to 49 Users
	· 1 Manager
· Up to 28 Users
	· 1 Master
· 1 Manager
· Up to 48 Users
	· Up to 2 Masters
· Up to 2 Managers
· 1 Override Manager
· 1 Administrator
· 89 Users

	Override user
	
	1 User*
	Up to 10 Users
	1 User*
	Up to 10 Users*
	Up to 80 of the users, available in groups*

	Time delay
	1-99 minutes
	1-99 minutes
	1-99 minutes
	1-99 minutes
	1-99 minutes
	1-99 minutes
Variable Time Delay*

	Dual mode*
	
	Available
	Available
	Available
	Available
	Available (in groups)

	Dallas keys*
	
	Available
	Available
	Available
	Available
	Available

	Audit*
	
	100 events
w/o time and date
	· Up to 8.000 events with time&date
· Automatic DST
	· Up to 8.000 events with time&date
· Audit display
· Automatic DST
	· Up to 11.000 events with time&date
· Audit display
· Automatic DST
	· Up to 15.000 events with time&date
· Audit display
· Automatic DST

	Interface*
	
	· Silent alarm
· Remote disable opening
	· Silent alarm
· Remote disable opening
· Remote time delay override
	· Silent alarm
· Remote disable opening
· Remote time delay override
	· Silent alarm 
· Remote disable opening
· Remote time delay override
	· Silent alarm
· Remote disable functions
· Remote management (TCP/IP, RS485)

	Time lock
	
	
	
	
	· Weekly opening and closing
· 60 between closing and opening periods
· Immediate & temporary time lock 
· Time programmed from the keypad or a PC
	· 3 users tables, each with weekly opening and closing
· 60 between closing and opening periods
· Immediate & temporary time lock
· Time programmed from the keypad or a PC
· Opening extensions

	Advanced features*
	· Backlit keypad (Pulse Next)
· Slim version (Pulse Next)

	· Backlit keypad (Pulse Next)
· Slim version (Pulse Next)
	· Battery level test
· Fully configurable by keypad (more than 80 configurations)
· Codes expiry*
· Door open alarm*
· Bolt status output*
· ERC – Emergency Rescue Code*
	
	· Dynamic Codes
· Multiple locks: 2
	· Dynamic codes
· Codes expiry
· Multiple locks: 15

	Certifications
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All locks systems have penalty and low battery warning
*Optional features available with additional hardware and/or as a programming request when purchased
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